# MB_CommBootRequestAll

## C Specification

  `#include <nitro/mb.h>`
  `BOOL MB_CommBootRequestAll(void);
  `

## Arguments

None.

## Return Values

Returns TRUE if a boot request is successfully sent to all children. Otherwise, it returns FALSE.

## Description

This sends a boot request to all children that are multiboot processing with the current parent. It returns TRUE if it has already received a boot possible notification from all children, and if it can successfully send a boot request to all of these children.

## See Also

`MBCommPState, MB_CommBootRequest MB_CommGetParentState MB_CommGetChildUser MB_StartParent MB_End
`

## Revision History

09/09/2004 Initial version.

CONFIDENTIAL