# RTCAlarmChan

## Definitions

  `#include <nitro/rtc.h>`

      typedef enum
      {
      	RTC_ALARM_CHAN_1 = 0 ,
      	RTC_ALARM_CHAN_2 ,
      	RTC_ALARM_CHAN_MAX

      } RTCAlarmChan;

## Elements

RTC_ALARM_CHAN_1 | Alarm Channel #1.
RTC_ALARM_CHAN_2 | Alarm Channel #2.

## Description

There are two alarm channels that you can register in the real time clock. Although each channel can operate independently, there is only one interrupt output common to both. Therefore, if interrupts are simultaneously generated in two channels, only one interrupt will be generated.

## Revision History

03/08/2005 Standardized the Japanese term for "interrupt"
05/18/2004 Initial version

CONFIDENTIAL