# TP_RequestAutoSamplingStopAsync

## C Specification

  `#include <nitro/spi.h>`

      void TP_RequestAutoSamplingStopAsync( void );

## Arguments

None.

## Return Values

None.

## Description

This function asynchronously issues a request to ARM7 to stop autosampling touch panel values.

In this function, you must confirm whether the request to ARM7 was properly processed. To obtain the success or failure of the request, you can either first use `TP_WaitBusy` to wait for completion and then use `TP_CheckError`, or if a user callback has been set in `TP_SetCallback`, use an argument.

## See Also

`TP_RequestAutoSamplingStart`, `TP_WaitBusy`, `TP_CheckError`, `TP_RequestAutoSamplingStop`

## Revision History

04/21/2004 Initial version

CONFIDENTIAL