# TP_GetUnCalibratedPoint

## C Specification

  `#include <nitro/gx/gx_bgcnt.h>`

      void TP_GetUnCalibratedPoint( u16 * raw_x,
                                        u16 * raw_y,
                                        u16 dx,
                                        u16 dy );

## Arguments

raw_x, raw_y | Pointer used for acquiring touch panel value results
dx, dy | Screen coordinates

## Return Values

None.

## Description

This function uses the calibration values that were set by `TP_SetCalibrateParam` to inverse-transform from screen coordinates to raw touch panel values. If no calibration parameters are set, screen coordinates are output unchanged.

## See Also

`TP_SetCalibrateParam`, `TP_GetCalibratedPoint`

## Revision History

04/16/2004 Initial version

CONFIDENTIAL