# CARD_TryWaitRomAsync

## C Specification

  `#include <nitro/card.h>`
  `BOOL CARD_TryWaitRomAsync(void);`

## Arguments

None

## Return Values

Returns `FALSE` if an asynchronous function that operates on a CARD ROM device is actively calling and processing is not yet complete. Otherwise it returns `TRUE`.

## Description

Determines whether or not an asynchronous process to a ROM device is complete. Regardless of the status of the target process, the function immediately returns a value.

## See Also

`CARD_ReadRomAsync, CARD_WaitRomAsync`

## Revision History

07/05/2004 Initial version

CONFIDENTIAL