MI_GetCartridgePriority

# MI_GetCardProcessor

## C Specification

  `#include <nitro/mi.h>`
  `MIProcessor MI_GetCartridgeProcessor( void )`

## Arguments

None.

## Return Values

Settings for access permission to the cartridge.

## Description

This function acquires the permission settings to access AGB compatible 32-pin cartridge slot hardware. The return value is an `MIProcessor` array type that has the following meanings:

`MI_PROCESSOR_ARM9` | Sets access permission to ARM9.
`MI_PROCESSOR_ARM7` | Sets access permission to ARM7.

## Internal Operation

Accesses the `EXMEMCNT` I/O register `(0x4000204)`.

## See Also

`None.
`

## Revision History

10/18/2004 Corrected the return value text.
01/14/2004 Function name changed from `MI_GetCartridgePriority`.
01/14/2004 enum name changed to `MIProcessor`.
12/18/2003 Initial version.

CONFIDENTIAL