# MI_*ToH*

## C Specification

  `#include <nitro/mi.h>`
  `#define MI_LEToH8(val) (val)
  #define MI_BEToH8(val) MI_SwapEndian8(val)
  #define MI_LEToH16(val) (val)
  #define MI_BEToH16(val) MI_SwapEndian16(val)
  #define MI_LEToH32(val) (val)
  #define MI_BEToH32(val) MI_SwapEndian32(val)
  `

## Arguments

val | The value whose endianity is to be converted. Note: Because this is a macro, evaluation is performed several times.

## Return Values

Returns a value converted from the specified endianity (`u16 or u32`).

## Description

This macro converts the specified value from the specified endianity to the current environment. LE represents little-endian, while BE represents big-endian.
Because the Nintendo DS uses a little-endian environment, this macro does nothing when LE is specified.
Note: Because this is a macro, arguments are evaluated several times.

These 8-bit versions do not actually perform any conversions, but they have been included for source code uniformity.

## See Also

`MI_SwapEndian* MI_Load* MI_Store* MI_HTo*`

## Revision History

04/05/2006 Initial version.

CONFIDENTIAL