# GXS_EndLoadBGExtPltt

## C Specification

      #include <nitro/gx/gx_load.h>

      void GXS_EndLoadBGExtPltt(void);

## Arguments

None.

## Return Values

None.

## Description

This function is called after transferring the BG palette data to the sub 2D Engine BG Extended palette. Internally, the VRAM bank that was allocated to LCDC by `GXS_BeginLoadBGExtPltt` is restored to the sub 2D Engine BG Extended palette data.

## See Also

`GXS_BeginLoadBGExtPltt`, `GXS_LoadBGExtPltt`

## Revision History

02/09/2004 Initial version.

CONFIDENTIAL